Fabrication notes for <Board 1 – Pad and Pogo Pin>

**Designer contact: Jacky Li,** [**jackymengyangli@uchicago.edu**](mailto:jackymengyangli@uchicago.edu)

**Board Stack Info:** 2 layer board, 1.6 mm thickness, 1/1 oz Cu. Size 9.65 \* 11.79 in.

No impedance control needed on this board.